|  |  |
| --- | --- |
| DOTLOGO2 |  **Illinois Modified AASHTO R 60 Checklist** **Sampling Fresh Concrete** |
|  |
| Note: Illinois Modified AASHTO R 60 is formerly Illinois Modified AASHTO T 141. |
|  |
| The following is a summary checklist of the key steps involved in sampling freshly mixed concrete. |
|  |
| **Did the tester:** |  | **YES** | **NO** |  |
|  |
| 1. | Sample the concrete after discharge of at least 4 ft3 (0.1 m3) of concrete?  | [ ]  | [ ]  |  |
|  |
| 2. | Repeatedly pass a receptacle through the entire discharge stream, or completely divert the discharge stream into a sampling container?  | [ ]  | [ ]  |  |
|  |
| 3. | Remix the concrete with a damp shovel?  | [ ]  | [ ]  |  |
|  |
| 4. | Obtain the sample within a 15 minute interval?  | [ ]  | [ ]  |  |
|  |
| 5. | Start tests for slump and air within 5 minutes after the final portion of the sample was obtained?  | [ ]  | [ ]  |  |
|  |
| 6. | Start molding cylinders or beams within 15 minutes after the sample was fabricated?  | [ ]  | [ ]  |  |
|  |
| 7. | Protect the sample against contamination and rapid evaporation?  | [ ]  | [ ]  |  |
|  |
| Tester: |       | Observer: |       | Date: |       |
|  |
| REMARKS: |       |
|  |       |
|  |       |
|  |       |