|  |  |
| --- | --- |
| DOTLOGO2 |  **Illinois Modified AASHTO T 152 Checklist** **Air Content of Freshly Mixed Concrete by the Pressure Method, Type A Meter** |
|  |
| The following is a summary checklist of the key steps involved in determining the air content of freshly mixed concrete by the pressure method, using the Type A meter. |
|  |
| **Did the tester:** |  | **YES** | **NO** |  |
|  |
| 1. | Dampen the inside of the air meter bowl and top, the hand scoop or trowel, the tamping rod, and the strike-off bar?  | [ ]  | [ ]  |  |
|  |
| 2. | Fill the bowl in three equal layers by volume, slightly overfilling the top layer?  | [ ]  | [ ]  |  |
|  |
| 3. | Rod each layer 25 times with the hemispherical end of the tamping rod, uniformly distributing the strokes?  | [ ]  | [ ]  |  |
|  |
| 4. | Rod the bottom layer throughout its depth, without forcefully striking the bottom of the bowl?  | [ ]  | [ ]  |  |
|  |
| 5. | Rod the middle and top layers about 1 in. (25 mm) into the underlying layer?  | [ ]  | [ ]  |  |
|  |
| 6. | Tap the sides of the bowl smartly 10-15 times with the mallet after rodding each layer?  | [ ]  | [ ]  |  |
|  |
| 7. | Strike off the concrete level with the top of the bowl using the strike-off bar and clean off the rim?  | [ ]  | [ ]  |  |
|  |
| 8. | Clean and moisten the inside of the cover before clamping it to the base?  | [ ]  | [ ]  |  |
|  |
| 9. | Add water through the funnel valve until the level was slightly above the index mark, or until water flowed from the upper petcock?  | [ ]  | [ ]  |  |
|  |
| 10. | Adjust the bottom of the meniscus (water level) to be level with the index mark?  | [ ]  | [ ]  |  |
|  |
| 11. | Close the funnel valve and upper petcock and apply pressure using the hand pump?  | [ ]  | [ ]  |  |
|  |
| 12. | Read the air content at 15 psi (103 kPa), or apply the proper multiplication factor (1.25 or 2.00) if the test was conducted at 10 or 5 psi (69 or 34 kPa), respectively?  | [ ]  | [ ]  |  |
|  |
| 13. | Calculate and record the air content to the nearest tenth of a percent?Air Content = Gauge Reading - Aggregate Correction Factor  | [ ]  | [ ]  |  |
|  |
| Tester: |       | Observer: |       | Date: |       |
|  |
| REMARKS: |       |
|  |       |
|  |       |
|  |  |