|  |  |
| --- | --- |
| LOGO2LIN |  Soil Boring Log |
| Route: |       |  Structure No.: |       | (Exist.) |       | (Prop.) |  | Date: |       |  Page: |    |  of |    |
|  |
| Section: |       |  Description:  |       |
|  |
| County: |       |  Drilling Method: |       |  Hammer Type: |  |
|  |
| Boring No.: |        |  | Logged by:  |       |
|  |
|  | Station: |       |  | ELE V. | DEP**T****H** | BLO**W****S** | U.C.S.**Qu** | **M**OIS T. |  Surface Water Elev.: |       | ft | ELE V. | DEP**T****H** | BLO**W****S** | U.C.S.**Qu** | **M**OIS T. |
|  | Offset: |       |  |  |  |  |  |  |  Groundwater Elev. |  |  |  |  |  |
|  | Latitude: |       |  |  |  |  |  |  |   | First Encounter: |       |  ft |  |  |  |  |  |
|  | Longitude: |       |  |  |  |  |  |  |   | Upon Completion: |       |  ft |  |  |  |  |  |
|  | Ground Surface El.: |        |  ft |  |  |  |  |  |  | After |       | Hours |       |  ft |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
| Soil Type, Description & Observations |  |  |  |  |  | Soil Type, Description & Observations |  |  |  |  |  |
|  | (ft) | (ft) | /6 in. | (tsf) | (%) |  | (ft) | (ft) | /6 in. | (tsf) | (%) |
|        |  |      |      |      |       |  |       |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  -5 |      |      |      |       | -25 |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       | -10 |      |      |      |       | -30 |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |            |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       | -15 |      |      |      |       | -35 |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       |  |      |      |      |       |  |      |      |      |
|       | -20 |      |      |      |       | -40 |      |      |      |
| The U.C.S. Qu column represents the Unconfined Compressive Strength using either the IDOT Rimac Test Procedure or AASHTO 208.The Qu failure mode is indicated by B for Bulge or S for Shear. P is shown when sample disturbance only allows Penetrometer testing.The Standard Penetration Test (SPT) N value is the sum of the second and third Blows /6 in. values in each sample using AASHTO T 206. |  |  |  |  |  |  |      |