|  |  |
| --- | --- |
| DOTLOGO2 | **White Pavement Marking Paint****Certification Statement** **(Waterborne Type)** |
|  |
| Inspector SSN | 500000000 | Type of Inspection | PRO | Total Samples | 01 |  |
|  |
| Resp Org: Loc | 50 | Lab | PP | Name |       |  |
|  |
| Producer Code |       | Name |       | Location |       |  |
|  |
| Test ID No.  |       |  |
| (To be entered by IDOT) |
|  |
| Date Sampled |       |  |
|  |
| Sequence Number |       |  |
|  |
| Material Code | 40444 |  |
|  |
| Material Name | WPMP |  |
|  |
| Quantity Tested |       | Drums |       | GAL |
|  |
|  |       | Totes |       | GAL |
|  |
|  |       | Pails |       | GAL |
|  |
| Batch Number |       |  |
|  |
| TRAFFIC PAINT TEST RESULTS |
|  |
|  | Specs |
|  |
| **Weight/Gallon at 25ºC** |   .   | lbs |       |  |
|  |
| Density at 25ºC |  .    | kg/L |       |  |
|  |
| Viscosity at 25ºC |    | KU | 83-98 |  |
|  |
| Drying Time, no pickup |   | minutes | 10 | max |
|  |
| Fineness of Grind |   |  | 3 | min |
|  |
| Daylight Reflectance (Y value) |   .  | % | 85 | min |
|  |
| Non-volatile (Total Solids) |   .  | % | 73 | min |
|  |
| Vehicle non-volatile |   .  | % | 44 | min |
|  |
| Pigment |   .  | % | 50-54 |  |
|  |
| Vehicle |   .  | % | 46-50 |  |
|  |
| Contrast Ratio |  .    |  | 0.97 | min |
|  |
| Tested By |       | Date |       |  |
|  (Name) |
|  |
| This certifies that above material meets all the requirements of the Illinois Department of Transportation’s Standard Specifications for Road and Bridge Construction, Article 1095.02. |
|  |
|  |  |  |
|  Certified By |
|  (Signature) |
|  |