|  |  |
| --- | --- |
| DOTLOGO2 |  **Illinois Test Procedure SCC-6 Checklist** **Static Segregation of Hardened Self- Consolidating Concrete Cylinders** |
|  |
| The following is a summary checklist of the key steps involved in making self-consolidating concrete cylinder specimens. |
|  |
| **Did the tester:** |  | **YES** | **NO** |  |
|  |
| 1. | Place the molds on a flat, level, firm surface which was free of vibration or other disturbances?  | [ ]  | [ ]  |  |
|  |
| 2. | Fill the mold in one lift, slightly overfilling the top layer?  | [ ]  | [ ]  |  |
|  |
| 3. | Strike off the surface with a tamping rod or strike-off bar to produce a flat and even surface, using a minimum amount of manipulation?  | [ ]  | [ ]  |  |
|  |
| 4. | Cover the specimens with a plastic cylinder lid or with a plastic sheet secured by a rubber band?  | [ ]  | [ ]  |  |
|  |
| 5. | Identify the specimen by writing on the outside of the mold?  | [ ]  | [ ]  |  |
|  |
| 6. | Place the specimens where they could remain undisturbed, and within the curing temperature range of 60° F to 80° F (16° C to 27° C)?  | [ ]  | [ ]  |  |
|  |
| 7. | Cure the specimens for a minimum 24 ± 0.5 hours ***or*** ensured a minimum compressive strength of 900 psi (6200 kPa)?  | [ ]  | [ ]  |  |
|  |
| 8. | Saw cut the specimens lengthwise down the center?  | [ ]  | [ ]  |  |
|  |
| 9. | Make a visual assessment of the cut plane of the hardened concrete cylinder according to the Hardened Visual Stability Index (HVSI)?  | [ ]  | [ ]  |  |
|  |
|  |
| Tester: |       | Observer: |       | Date: |       |
|  |
|  |
| REMARKS: |       |
|  |
|  |       |
|  |
|  |       |
|   |
|  |       |