|  |  |
| --- | --- |
| DOTLOGO2 | **Glass Beads for Pavement Markings****Certification Statement** |
|  |
|  |
| Inspector SSN | 500000000 | Type of Inspection | PRO | Total Samples | 01 |  |
|  |
| Resp Org | 50 | Lab | PP | Name |       |  |
|  |
| Producer Code |       | Name |       | Location |       |  |
|  |
| Test ID No. |       |  |
| (To be entered by IDOT) |
|  |
| Date Sampled |       |  |
|  |
| Sequence Number |       |  |
|  |
| Material Code | 60401 |  |
|  |
| Material Name | Glass Beads |  |
|  |
| Quantity Tested |       | Totes/Box |       |  |
|  |
|  |       | Bags |       |  |
|  |
| Batch Number |       |  |
|  |
| GLASS BEAD TEST RESULTS |
|  |
| **Gradation (Percent Passing)** | Specs |
|  |
| Sieve 20/850µm |       | % |  | 100 |  |
|  |
| Sieve 30/600µm |       | % |  | 75-100 |  |
|  |
| Sieve 50/300µm |       | % |  | 15-40 |  |
|  |
| Sieve 100/150µm |       | % |  | 0-5 |  |
|  |
| Sieve 200/75µm |       | % |  | 0-1 |  |
|  |
| Imperfections |       | % |  | 20 | max |
|  |
| Index of Refraction |       |  | 1.50 | min |
|  |
| Flowing Properties |       |  | PASS |  |
|  |
| Tested By |       | Date |       |  |
|  (Name) |
|  |
| This certifies that above material meets all the requirements of the Illinois Department of Transportation’s Standard Specifications for Road and Bridge Construction, Article 1095.07. |
|  |
|  |  |  |
|  Certified By (Signature)  |
|  |